**Maintenance Procedure for Kalingastone Engineered Terrazzo**

|  |
| --- |
| **Daily Maintenance** |
| * **Wet mopping to be done by using Crystal Clean of Akemi / Stone & Tile Cleaner of DuPont / Equivalent (2 caps of Crystal Clean of Akemi in one bucket of water – 5 Litres).** * **The mop should be clean and wringed properly before applying at all the time. (Water should not drip from the mop)** |
| * **The dirty mop should be cleaned in a separate bucket of water always before dipping in the bucket comprising Crystal Clean of Akemi/Equivalent Cleaner.** |
| * **The Floor should be finally cleaned with plain water.** |

|  |
| --- |
| **As & When Required** |
| * **Deep cleaning to be done with a soft brush / Red Buffing Pad using Crystal Clean of Akemi / Stone & Tile Cleaner of DuPont / Equivalent (2 caps of Crystal Clean / Stone & Tile cleaner in one bucket of water – 5 Litres).** * **Note : For deep / stubborn stains : Stone Cleaner of Akemi / DuPont’s KlenzAll Cleaner / Equivalent (2 caps of Stone Cleaner of Akemi / KlenzAll of DuPont / Equivalent in one bucket of water – 5 Litres) to be used, if required.** |
| * **Repeat cleaning the floor with plain water.** * **Vacuum the dirty water immediately.** * **Let the floor dry completely.** |
| * **After ensuring proper cleaning, apply approximately ½ cup shining powder (Crystallization) of DuPont / Equivalent plus 1 cup clean water to stone surface.** * **Refinish using single disc machine fitted with White pad. Keep compound wet while**   **refinishing with plenty of water. Add shining powder as needed.**   * **Refinish area until the desired level of shine has been achieved.** * **Rinse well and use a wet vacuum until to remove all remaining compound.** |
| * **Let the floor dry completely.** |